## Uses of Class
org.gicentre.utils.spatial.Ellipsoid

- Packages that use Ellipsoid
  Package | Description
  --- | ---
  org.gicentre.utils.spatial | Spatial and geographic utilities for use with Processing.

- - ### Uses of Ellipsoid in org.gicentre.utils.spatial

    Methods in org.gicentre.utils.spatial that return Ellipsoid
    Modifier and Type | Method and Description
    --- | ---
    `Ellipsoid` | WebMercator.`getEllipsoid()` Reports the ellipsoid used in the transformation.
    `Ellipsoid` | UTM.`getEllipsoid()` Reports the ellipsoid used in the transformation.
    `Ellipsoid` | Swiss.`getEllipsoid()` Reports the ellipsoid used in the transformation.
    `Ellipsoid` | ObliqueMercator.`getEllipsoid()` Reports the ellipsoid used in the transformation.
    `Ellipsoid` | LambertConformalConic.`getEllipsoid()` Reports the ellipsoid used in the transformation.
    `Ellipsoid` | FrenchNTF.`getEllipsoid()` Reports the ellipsoid used in the transformation (Clarke 1880).
    `Ellipsoid` | AlbersEqualAreaConic.`getEllipsoid()` Reports the ellipsoid used in the transformation.

    Constructors in org.gicentre.utils.spatial with parameters of type Ellipsoid
    Constructor and Description
    `AlbersEqualAreaConic(Ellipsoid ellipsoid, double lat1, double lat2)` Initialises the Albers converter with the given ellipsoid and standard parallels.
    `AlbersEqualAreaConic(Ellipsoid ellipsoid, double lat1, double lat2, double lon0, double lat0, double falseEast, double falseNorth)` Initialises the Albers converter with the given ellipsoid.
    `LambertConformalConic(Ellipsoid ellipsoid, double lat1, double lat2, double lon0, double lat0, double falseEast, double falseNorth)` Initialises the projection converter with the given ellipsoid.
    `ObliqueMercator(Ellipsoid ellipsoid)` Initialises the Oblique Mercator converter with the given ellipsoid.
    `UTM(Ellipsoid ellipsoid, float lat, float lng)` Initialises the UTM converter with the given ellipsoid.
    `UTM(Ellipsoid ellipsoid, int zoneNumber, char zoneLetter)` Initialises the UTM converter with the given ellipsoid and zone.